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Acknowledgement of Country

Yarra Ranges Council acknowledges the Wurundjeri and other Kulin Nations as the Traditional Owners and Custodians of these lands and waterways. We pay our respects to all Elders, past, present, and emerging, who have been, and always will be, integral to the story of our region. We proudly share custodianship to care for Country together.
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	Arterial Road
	Refers to freeways, highways and declared main roads, which are managed by the Victorian Government, through Head Transport for Victoria (as the co-ordinating road authority).


	Co-ordinating road authority
	The organisation which has the responsibility to co-ordinate works. Generally, if the road is a freeway or arterial road, this will be Head Transport for Victoria. Generally, if the road is a municipal road, this will be Council.


	Council
	Refers to the Yarra Ranges Council


	Demarcation agreement
	An agreement between Council and another organisation that defines areas of responsibility for boundary roads.


	Motor vehicle
	Refers to a vehicle that is propelled by an in-built motor and is intended to be used on a roadway. This does not include a motorised wheelchair or mobility scooter which is incapable of travelling at a speed greater than 10 km/h and is solely used for the conveyance of an injured or disabled person.


	Municipal road(s)
	Road for which the municipal council is the co-ordinating road authority.  The Road Management Act 2004 imposes specific duties on the municipal council with respect to the inspection, repair and maintenance of these roads and associated road-related infrastructure.


	Non-road infrastructure
	Refers to infrastructure in, on, under or over a road, which is not road infrastructure. This includes (but is not limited to) such items as gas pipes, water and sewerage pipes, cables, electricity poles and cables, tram wires, rail infrastructure, bus shelters, public telephones, mail boxes, roadside furniture and fences erected by utilities, or providers of public transport.


	Other roads
	Include roads in state forests and reserves, and roads on private property. Municipal councils are not responsible for the inspection, repair or maintenance of these roads.


	Pathway
	Where located in road reserve treated as a general or high use footpath. Where located outside the road reserve treated as a trail under Paths and Trails Plan.


	Plan
	Refers to this Road Management Plan.


	Public Road
	As defined by the Road Management Act 2004 and includes a freeway, an arterial road, a municipal road declared under section 14(1) of the Act and a road in respect of which Council has made a decision that it is reasonably required for general public use and is included on the Register of Public Roads.


	Road
	Has the same meaning as in the Road Management Act 2004, being inclusive of any public highway, any ancillary area and any land declared to be a road under section 11 of that Act or forming part of a public highway or ancillary area.


	Road infrastructure
	Refers to infrastructure which forms part of a roadway, pathway or shoulder, which includes structures and materials.


	Road-related infrastructure
	Refers to infrastructure installed or constructed by the relevant road authority to either facilitate the operation or use of the roadway or pathway, or support or protect the roadway or pathway.


	Road Reserve
	Refers to the area of land that is within the boundaries of a road.
Example: any nature strip, forest, bushland, grassland or landscaped area within the road reserve would be roadside. 


	Roadside
	Refers to any land that is within the boundaries of the road (other than shoulders) which is not a roadway or pathway. This includes land on which any vehicle crossing or pathway, which connects from a roadway or pathway on a road to other land, has been constructed.
Example: any nature strip, forest, bushland, grassland or landscaped area within the road reserve would be roadside.


	Roadway
	Refers to the area of a public road that is open to, or used by, the public, and has been developed by a road authority for the driving or riding of motor vehicles. This does not include a driveway providing access to a public road, or other road, from adjoining land.


	Shoulder
	Refers to the cleared area, whether constructed or not, that adjoins a roadway to provide clearance between the roadway and roadside. This does not refer to any area that is not in the road reserve.
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[bookmark: _Toc152582059][bookmark: _Toc152584802][bookmark: _Toc204352583]1.1	Purpose of this Plan

Section 50 of the Road Management Act 2004 sets the following objectives for a municipal road management plan:

1) To establish a system for our road management functions, which is based on policy, operational objectives and available resources.
2) To set a performance standard for our road management functions.

Although termed a ‘plan’ in the Road Management Act 2004, it is functionally an operational protocol, describing the systems and rules used to make decisions and meet objectives within our available resources. The plan forms part of Council’s larger Asset Management Framework related to maintenance and operations.

This Plan is the Road Management Plan for the purposes of s.39 of the Road Management Act 2004.
[bookmark: _Toc152582060][bookmark: _Toc152584803]
[bookmark: _Toc204352584]1.2	Legislation guiding this Plan

In addition to the Road Management Act 2004, this Plan also has regard to the following legislation, regulation and codes of practice:

· Local Government Act 2020 
· Ministerial Codes of Practice under the Road Management Act 2004
· Road Management (General) Regulations 2016 
· Road Management (Works and Infrastructure) Regulations 2015 
· Road Safety Act 1986 
· Wrongs Act 1958.
[bookmark: _Toc152582061][bookmark: _Toc152584804]
[bookmark: _Toc204352585]1.3	What is covered in this Plan?

The Plan is divided into six sections:

1. Introduction.
2. Rights and Responsibilities – Legislation and local laws relevant to road management.
3. Road Management Systems - How we classify roads, streets and footpaths – known as our asset hierarchy – and the plans and processes we use to maintain roads and road-related infrastructure.
4. Register of Public Roads – What it contains, how to access and the process for making changes.
5. Technical References. 
6. Attachments:
a. Attachment 1, Road Hierarchy – Urban Roads
b. Attachment 2, Road Hierarchy – Rural Roads
c. Attachment 3, Pathway Hierarchy
d. Attachment 4, Inspection Requirements
e. Attachment 5, Inspection Frequencies
f. Attachment 6, Defect Intervention Levels and Repair Timeframes
[bookmark: _Toc152582062][bookmark: _Toc152584805]
[bookmark: _Toc204352586]1.4	Updating the Plan

This Plan must be updated within a set period following a Council election. Outside of this cycle, changes may be required from time to time.

The following process will be used to manage these changes:
· If material changes are made to standards and specifications, a report will be presented to Council, along with a brief explanation as to why such changes are necessary. The review process must follow the steps as set out in the Road Management (General) Regulations 2016 Part 3 – Road Management Plans.
        
These changes will be made in accordance with the processes prescribed by the Road Management Act 2004. To assist with version control, these changes must be numbered as follows:

· by whole numbers – for example, from Version 1.00 to 2.00;- or.
· by decimals – for example, from Version 1.00 to 1.01.

[bookmark: _Toc152582063][bookmark: _Toc152584806][bookmark: _Toc204352587]1.5	Exceptional Circumstances

Council will endeavour to meet its described tasks under this Plan.

However, there may be situations or circumstances that affect Council's business activities to the extent that it cannot deliver on the service levels of the Plan. These include but are not limited to: natural disasters, such as fires, floods, or storms, or a prolonged labour or resource shortage, due to a need to commit or redeploy Council staff and/or equipment elsewhere or due to the effects of pandemic and or government intervention.

[bookmark: _Toc152582064][bookmark: _Toc152584807][bookmark: _Toc204352588]1.5.1	Suspension of the Plan

In the event that the Chief Executive Officer (CEO) of Council has considered the impact of such an event on the limited financial resources of Council and its other conflicting priorities, and determined that the Plan cannot be met, then pursuant to Section 83 of the Wrongs Act 1958, the CEO will write to Council’s Officer in charge of the Plan and inform them that some, or all, of the timeframes and responses in Council’s Plan are to be suspended.

[bookmark: _Toc152582065][bookmark: _Toc152584808][bookmark: _Toc204352589]1.5.2	Reinstatement of the Plan

Once the scope of the event/s have been determined, and the resources committed to the event response have been identified, then there will be an ongoing consultation between Council’s CEO and Council’s Officer responsible for the Plan, to determine which parts of Council’s Plan are to be reactivated and when.

[bookmark: _Toc152582066][bookmark: _Toc152584809][bookmark: _Toc204352590]1.5.3	Communication and documentation around Plan suspension

Council will provide information/statements to residents about the suspension or reduction of the services under its Plan, including:

· How the work that will be done has been prioritised; and
· The period for which it is likely to be affected.

This information will be provided by the Council on its website where this Plan is located and other media as appropriate. 
Where Council has suspended, in part or whole, the operation of this Plan, associated documents, concerning such suspension (for example communications, meeting minutes, schedules) will be recorded and stored.

[bookmark: _Toc204352591][bookmark: _Toc152582067][bookmark: _Toc152584810]1.5.4	Inspections and repairs during suspension 

The suspension of this Plan will not necessarily mean that all inspections and repairs halt. However, it may mean that only certain categories of inspections and repairs are undertaken. These will be based on a risk assessment and resources available to the Council, taking into account the resources needed to address the impact of the trigger event. For example, some reactive inspections may take place and repair (temporary or permanent) of roads/footpaths which pose a high risk may be undertaken, depending on the resources available to Council and the accessibility of each asset.
[bookmark: _Toc152582068][bookmark: _Toc152584811]
[bookmark: _Toc204352592]1.6	Responsibility for the Plan

The Council Officer responsible for administering and implementing is the Director Built Environment and Infrastructure or a person acting in the role, or a renamed version of that role.

[bookmark: _Toc152582069][bookmark: _Toc152584812]

[bookmark: _Toc204352593]Rights and Responsibilities
2.1 [bookmark: _Toc152582070][bookmark: _Toc152584813][bookmark: _Toc204352594] Public Roads

Public roads are defined in the Road Management Act 2004 as including:

· a freeway
· an arterial road
· a road declared under section 204(1) of the Local Government Act 1989
· a municipal road declared under section 14(1) of the Road Management Act 2004
· a road in respect of which Council has made a decision that it is reasonably required for general public use and is included on the Register of Public Roads.

[bookmark: _Toc152584814][bookmark: _Toc204352595]2.2	Key stakeholders

Key stakeholders impacted by this Plan include:

· the general community (for recreation, sport, leisure and business)
· residents and businesses adjoining the road network
· pedestrians
· vehicle users with motorised vehicles, such as trucks, buses, commercial vehicles, cars and motorcycles
· users of smaller, lightweight vehicles, such as pedal-powered bicycles, motorised buggies, wheelchairs, prams and so on
· tourists and visitors to the area
· emergency agencies (Victoria Police, Country Fire Authority, Ambulance Victoria, State Emergency Services)
· the military (in times of conflict and emergency)
· traffic and transportation managers
· managers of the road network asset
· construction and maintenance personnel, who build and maintain asset components
· utility agencies using the road reserve for infrastructure (water, sewerage, gas, electricity, telecommunications)
· state and federal governments, who periodically provide funding for roads.

2.3 [bookmark: _Toc152584815][bookmark: _Toc204352596] Coordinating & Responsible Road Authority

Section 35 of the Road Management Act 2004 provides that a road authority has power to do all things necessary or convenient to be done for or in connection with the performance of its functions under the Act.

Section 36 of the Road Management Act 2004 outlines which road authority is the coordinating road authority, namely: 

If the road is a municipal road, the municipal council of the municipal district in which the road or part of the road is situated.

However, there are instances where several authorities are responsible for parts of the road within the road reserve. Section 37 of the Road Management Act 2004 identifies who is the responsible road authority in particular circumstances.
[bookmark: _Toc152584816][bookmark: _Toc204352597]2.4	General Functions of a Road Authority

The general functions of a road authority are described within Section 34 of the Road Management Act 2004.

[bookmark: _Toc152584817][bookmark: _Toc204352598]2.5	Rights of the Road User

The rights of public road users, which are legally enforceable, are set out in Sections 8 to 10 of the Road Management Act 2004.

[bookmark: _Toc152584818][bookmark: _Toc204352599]2.6	Obligations of Road Users

[bookmark: _Toc152584819][bookmark: _Toc204352600]2.6.1	General Usage

The common law requires that a road user must take reasonable care for their own safety (see Ghantous v Hawkesbury City Council)

The Road Safety Act 1986 sets out obligations on road users, including section 17A which requires that a person who drives a motor vehicle on, or uses, a highway must drive in a safe manner have regard for all relevant factors, including without limiting their generality, the following:

(a) physical characteristics of the road
(b) prevailing weather conditions
(c) level of visibility
(d) the condition of any vehicle the person is driving or riding on the highway
(e) prevailing traffic conditions
(f) the relevant road laws and advisory signs
(g) the physical and mental condition of the driver or road user.

Section 17A of the Road Safety Act 1986 also requires that a road user must take reasonable care:

1. to avoid any conduct that may endanger the safety or welfare of other road users.
1. to avoid any conduct that may damage road infrastructure and non-road infrastructure on the road reserve.
1. to avoid conduct that may harm the environment of the road reserve.

[bookmark: _Toc152584820][bookmark: _Toc204352601]2.6.2	Incident Claims
	
If a person proposes to make a claim in relation to a public road or infrastructure for which Council is the responsible road authority, that person should contact Council. Where warranted (which will be on most occasions) Council will investigate and report the claim for insurance purposes.

Section 110 of the Road Management Act 2004 provides Council is not liable for property damages where the value of the damage is equal to or less than the adopted Threshold Amount.

In cases where the claim relates to assets Council does not own or is not responsible for in or on the road reserve, the person intending to make the claim must be advised and that person may choose to make such claim to the relevant person or authority.

[bookmark: _Toc152584821][bookmark: _Toc204352602]2.6.3	Permits for work within a road reserve

In cases where an individual or organisation proposes to carry out works within the road reserve that may impede public access, or interfere with road infrastructure, they must apply for a ‘works within road reserve’ permit. There are some exemptions, as noted in the Road Management (Works and Infrastructure) Regulations 2015.

Local laws also require property owners to apply for a vehicle crossing permit if they plan to build a driveway.

In both cases, a fee applies to cover the costs of the administration and inspection of the work.

[bookmark: _Toc152584822][bookmark: _Toc204352603]2.6.4	Obligation of others

There are several assets within the road reserve that Council does not have an obligation to inspect and/or maintain. These include:

· Non-road infrastructure – This includes (but is not limited to) such items as gas pipes, water and sewerage pipes, cables, electricity poles and cables, tram wires, rail infrastructure, bus shelters, public telephones, mail boxes, roadside furniture and fences erected by utilities, or providers of public transport.

· Vehicle driveways – This includes the crossover (and footpaths), together with associated drainage, pipeline and culverts located between the carriageway and the property boundary. This is the responsibility of the adjoining property owner. 

· Single property stormwater drains – for drains constructed within the reserve that carry water from a single property to an outlet in the kerb, or other drain.

· Utilities – including, but not limited to; telecommunication, power, water, gas and rail authority assets.

· Roadside – as per Section 107 of the Road Management Act, Council has no “statutory duty or a common law duty to perform road management functions in respect of a public highway which is not a public road or to maintain, inspect or repair the roadside”, described as “any land that is within the boundaries of the road (other than shoulders) which is not a roadway or pathway”.  This includes landscaped tree plots within the footpath/pathway where the surface of the tree plot is not constructed with the intention of providing a trafficable pedestrian surface.
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On sealed roads the Council is responsible for the maintenance of:
· Footpath
· Kerb & channel
· Road surface
· Councils’ drainage assets (excluding private property stormwater pipes within the road reserve)
· Guard rails, speed humps, signage, line marking and vegetation.

The property owner/occupier is responsible for:
· Construction, repair, replacement and maintenance of crossover
· Drainage (including pipes) under or within the crossover area
· Culverts
· Maintenance of naturestrip 
· Private property stormwater pipes within road reserve to the point of discharge. 
· Construction and maintenance of any footpaths to match existing footpaths.
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On unsealed roads the Council is responsible for the maintenance of:
· Road surface
· Open drain and other Council drainage assets (excluding private property stormwater pipes within the road reserve)
· Guard rails, speed humps, signage, line marking and vegetation.

 The property owner/occupier is responsible for:
· Construction, repair, replacement and maintenance of driveway crossover from the edge of the road to the property boundary including the culvert pipe, culverts and end walls
· Construction and maintenance of any footpaths to match adjacent footpath

Where Council becomes aware of a hazard created by the defective condition of assets / infrastructure owned by another party, Council may at its absolute discretion:

· If located within assets / infrastructure for which Council is responsible (e.g. footpaths, road surfaces, etc.), or otherwise presents an immediate and significant risk to members of the public, undertake temporary measures to reduce the risk to members of the public until such time as the respective owner can implement permanent repairs (subject also to Council’s available resources),
· Report in writing (e.g. email or letter) the presence of the hazard to the responsible party and request that repairs be implemented within a reasonable timeframe.
· Where repairs are not completed by the responsible party within the timeframe specified, Council may, subject to requirements, complete necessary repairs and invoice the responsible party for the costs.

However, where another party has a duty in relation to the asset / infrastructure, and Council has a discretionary power to take remedial action in relation to that matter, only that other party with the duty is liable in a subsequent proceeding, in accordance with s.104 of the Road Management Act 2004.
[bookmark: _Toc204352604]
Road Management Systems
[bookmark: _Toc152584824][bookmark: _Toc204352605]3.1	Background and Process

Road asset management involves managing both physical assets, and uses and operation that have the potential to impact their condition. It applies to all road assets, including:

· the road – pavement and surface, as well as footpaths, kerb and channel
· structures – bridges, culverts and traffic management devices
· road infrastructure – traffic signals and on-road electrical assets.

The aim of our road management system is to deliver a safe and efficient road network and meet community needs to the best of our ability, within available resources.

To create a road asset management system that would best meet our needs when inspecting, maintaining and repairing public roads, we used the following nationally recognised asset management frameworks:

· International Infrastructure Management Manual (IIMM) 2015, IPWEA
· IPWEA National Asset Management Systems (NAMS+)
· Other references, as listed in Technical References.

The system is designed to set the direction for our asset management activities. It is also linked to the annual business planning cycle.
[bookmark: _Toc152584825]
[bookmark: _Toc204352606]3.2	Asset Hierarchies – Municipal Road Network

Roads and footpaths within the municipal road network are classified according to a hierarchy that takes into account how they are used, who uses them and how often.
The hierarchy classification is used to determine the levels of service required, prioritise works programs and determine defect intervention responses.
The three levels in the hierarchy are:

1. Urban road & street network
Urban roads and streets are located in built up areas predominantly used for residential, commercial and industrial purposes.

This is further divided into two sub-categories:
· [bookmark: _Hlk197335181]Category 1: Local Access, less than 1,000 vehicles per day
· Category 2: Collector

See Attachment 1 for more information

2. Rural road network
Rural roads and streets are those that are not urban roads and streets as defined in Section 1 above.
This is further divided into two sub-categories:
· Category 1: Local Access, less than 1,000 vehicles per day
· Category 2: Collector
See Attachment 2 for more information
3. Pathway network
[bookmark: _Toc152584826]This is divided into two sub-categories, as follows:

Footpaths
· Category 1: General Use Areas
· Category 2: High Use Areas

Trodden paths and non-constructed paths are not Council assets and are not subject to the Road Management Plan.

Shared and Bicycle Pathways
Shared and Bicycle pathways are not subject to the Road Management Plan, unless located on a road reserve. These are managed in accordance with Council’s Paths and Trails Strategy. 

[bookmark: _Toc204352607]3.3	Our Road Network

More information about the Council’s Road network is shown in the tables below.

[bookmark: _Hlk201053778]Table 3.1 – Road length by hierarchy – date last updated:	 5/05/2025

	Hierarchy
	Length (km)
	% of Network

	Category 1: Local Rural
	745.5
	42.5

	Category 1: Local Urban
	503.5
	28.7

	Category 2: Collector Rural
	388.6
	22.1

	Category 2: Collector Urban
	115.3
	6.6

	Local Boundary Road
	0.3
	0.0

	Local Not Applicable
	1.7
	0.1

	Local Road Reserve
	0.4
	0.0

	Total
	1755.3
	100.0



Table 3.2 – Road Length by Surface Type – date last updated:	5/05/2025

	Surface Type
	Length (km)
	% of Network

	Sealed
	1061.1
	60.4

	Unsealed
	694.2
	39.6

	Without road pavement
	0.0
	0

	Total
	1755.3
	100.0



[bookmark: _Toc152584827][bookmark: _Toc204352608]3.4	Maintenance Management System

[bookmark: _Toc152584828][bookmark: _Toc204352609]3.4.1	Maintenance Management

Council has responsibilities to road users and the community to maintain public roads to a reasonably safe and suitable standard, within our available funds and resources. By developing long-term maintenance programs for our assets, we are better able to plan how we do this.

The following maintenance requirements shape our annual program and budget:

Routine maintenance standards
Standards vary across the network depending on the asset type and relevant risk factors, such as traffic volumes and composition, operating speeds, the susceptibility of assets to deterioration and the cost effectiveness of repairs. Competing priorities for funding are also relevant.

Defect intervention levels have been established using the VicRoads Standard Specification Section 750 and adapting it to local conditions.

The standards will be reviewed periodically to make sure they are adequate (see section 1.4).

Repair and maintenance works
Works must be completed within a specified time, depending on the severity and location of the defect. Response times are determined using local knowledge and experience and past performance as a guide. 

Response times are monitored and will be periodically reviewed (see section 1.4).

Temporary mitigation measures 
These are temporary works designed to reduce the risk of an incident, until such time as repair or maintenance works can be completed. 

Response times and safety measures – for example warning signs, flashing lights, and safety barriers – are determined by reference to the risk to safety, road type and traffic volume.

Emergency works 
Works that result from emergency incidents and must be undertaken immediately, for the safety of road users and the public. 

[bookmark: _Toc152584829]Emergency works might include traffic incident management, responses to fires, floods, storms and spillages, and any assistance required under the Victorian State Emergency Response Plan and Municipal Emergency Management Plan.

[bookmark: _Toc204352610]3.4.2	Asset Management Plans

Our asset management plans guide the development of long-term asset renewal programs, helping us to plan and finance asset renewal and replacement.

[bookmark: _Toc152584830][bookmark: _Toc204352611]3.4.3	Maintenance Surveys and inspections

A three-tier regime is used to inspect our road network assets. It covers safety issues, incidents, defects and condition inspections.

1. Reactive inspections (Request for Service or RFS)
These inspections are conducted in response to requests from the community. The inspection is carried out by both Council generally and Contractors and assessed according to the Hazard intervention levels, contained within Attachment 6.


2. Proactive Inspections
Regular timetabled inspections that are scheduled depending on traffic flow, the types of defects likely to impact the asset and the perceived risks of these defects.

3. Condition Inspections 
These inspections identify structural integrity issues which, if untreated, are likely to adversely affect the network overall. These issues may impact short-term serviceability, as well as the ability of the asset to perform for the duration of its intended life span.

Condition inspections are carried out on a three yearly schedule for roads and footpath assets. 


[bookmark: _Toc152584831][bookmark: _Toc204352612]3.4.4	Maintenance responsiveness and performance targets

The following information is recorded when Council receives a Request for Service (RFS) from the community:

· Date request received
· Name of person making the RFS
· Details of request, including location and nature of reported hazard/defect (including any specific measurements provided) and copies of any photographs provided, etc.
· The personnel / department to which the request has been assigned for action
· Date by which the request must be actioned (based on the target response times specified in Attachment 6); and
· After completion the date when the RFS was actioned and/or completed (this typically involves someone carrying out an RFS inspection, as described in section 3.4.3, followed by any necessary repair works).

By recording this information, Council can monitor compliance against target response times – that is, the time it takes from receiving an RFS to carrying out an inspection and ultimately completing necessary works.

An RFS will be inspected and assessed in accordance with timeframes specified in Attachment 6. Following are some possible outcomes from an RFS:

· If a defect identified exceeds a Description / Intervention Levels specified in Attachment 6, a work order will be created with a date for completion of works in line with respective specified repair timeframes.
· If repairs are significant – for example, rehabilitation works are required – temporary mitigation measures may be undertaken to reduce the risk posed by the hazard/defect until the complete works can be undertaken, this also subject to available resources.
· If the defect is assessed as below the Description / Intervention Level specified in Attachment 6, it will be recorded (including assessment level) and remedial action, such as a pre-emptive grind of a footpath joint, may or may not be conducted.

In all cases, the action taken must be recorded against the original RFS.

Target response times and intervention times are based on ‘normal’ conditions. The same level of service would not apply in cases where the Plan has been suspended, under Section 1.5.

[bookmark: _Toc152584832][bookmark: _Toc204352613]3.5	Asset Levels of Service

Five elements are taken into account when determining appropriate levels of service for the road network. These are:

· Community expectations;
· Technical standards;
· Organisational capacity;
· Performance measures and targets;
· Safety of road and footpath users.
[bookmark: _Toc152584833]

[bookmark: _Toc204352614]Register of Public Roads

Council maintains a register of public roads – called the Register of Public Roads – with the details of all public roads for which we are responsible. Ancillary areas such as carparks and wayside stops are not listed on the Road Register.

The Register of Public Roads is available on Council’s website. A hard copy can be inspected at our Customer Service Centres, listed below, on request.

	Location
	Address
	Phone number

	Civic Centre
	15 Anderson Street, Lilydale
	1300 368 333


	Monbulk Living and Learning Centre

	21 Main Road, Monbulk
	9756 7677

	Upwey Community Link

	40 Main Street, Upwey
	9752 6054

	Healesville Community Link

	110 River Street, Healesville
	5965 3501

	Upper Yarra Family Centre

	2444 Warburton Highway, Yarra Junction
	5965 3501



The Road Management Plan can also be viewed in PDF format on Council’s website:
www.yarraranges.vic.gov.au

[bookmark: _Toc152584834][bookmark: _Toc204352615]4.1	Maintenance Demarcation (Boundary) Agreements

Where there are boundary agreements between us and other road authorities or private organisations, the list of roads affected, and agreements, are listed in the Municipal Road Register.

Council has agreements with the following municipal road authorities:

· Maroondah
· Nillumbik 
· Cardinia 
· Casey
· Knox
· Manningham




The affected roads are:

	[bookmark: _Hlk195605351]BOUNDARY ROADS – CARDINIA AND YARRA RANGES 


	Road
	Section
	Distance (m)

	Duffys Road

	Start seal to road end
	872 Approximately


	Wellington Road
	Cardinia Creek Road to Aura vale Road

	2,262

	Aura Vale Road
	Wellington Road to Old Menzies Creek Road 
Surface unsealed

Selby Aura Road to Magpie Road

	444

	Old Menzies Creek Road
	Aura Vale Road to Selby Aura Road

	

	Selby Aura Road
	Old Menzies Creek Road to Aura Vale Road

	

	Magpie Road
	Aura Vale Road to end

	

	Kallista-Emerald Road
	Menzies Creek to Emerald-Monbulk Road

	

	Emerald-Monbulk Road
	Kallista-Emerald Road to Stewart Road

	190 Approximately


	Stewart Road
	Emerald-Monbulk Road to Paton Road

	

	Paton Road
	Stewart Road to Avonsleigh-Macclesfield-Woori Yallock Road

	

	Avonsleigh-Macclesfield-Woori Yallock Road
	Paton Road to Cherry Road


	

	Cherry Road
	Avonsleigh-Macclesfield-Woori Yallock Road to road forming Southern boundary Allotment 32

	

	Merritts Road
	Kennedy Road to Merritts Road

	







	BOUNDARY ROADS – CASEY AND YARRA RANGES 


	Road
	Section
	Distance (m)

	Horsewood Road
	Logan Park Road to Belgrave Hallam Road

	

	Belgrave Hallam Road
	Horsewood Road to Narre North Nursery boundary

	

	Boundary Road
	First bend to Berwick Road

Berwick Road to sharp bend

	




	BOUNDARY ROADS – KNOX AND YARRA RANGES 


	Road
	Section
	Distance (m)

	Pavitt Lane
	Liverpool Road to Sheffield Road
	775 Approximately


	Old Bayswater-Sassafras Road
	Fire Access Road 
	600 Approximately


	Basin-Olinda Road
	From Boundary to Ferndale Road
Surface unsealed

	400

	Ferndale Road
	Basin Olinda Road to bend

	1100 Approximately


	Mystic Road
	Natural Resources – Closed Off 

	

	Himalaya Road
	Natural Resources – Fire Access Road?

	

	The Boulevard
	Natural Resources – Fire Access Road?

	

	Victoria Street
	George Street to Grandview Crescent
	360 Approximately


	Fern Road
	New Road to Victoria Street
	260 Approximately


	New Road
	Fern Road to Glenfern Road
	740 Approximately


	Glenfern Road
	New Road to Lysterfield Road
	1108 Approximately


	Lysterfield Road
	Glenfern Road to Wellington Road
	4175 Approximately


	Wellington Road
	Lysterfield Road to Powells Road
	393 Approximately


	Powells Road
	Wellington Road to end
	350 Approximately


	School Road
	Natural Resources – Fire Access Road

	

	Burwood Highway (Monbulk Road)
	Mt. Dandenong Tourist Road to Ferny Creek Avenue 

Ferny Creek Avenue to UFTG postcode boundary

	210 Approximately

980 Approximately

	Royal Street
	From UFTG postcode boundary to Old Belgrave Road
	330 Approximately


	Old Belgrave Road
	Royal Street to Wynette Avenue

	129 Approximately


	Wynette Avenue
	Old Belgrave Road to George Street
	430 Approximately


	George Street
	Wynette Avenue to end of mountable kerb

From end of mountable kerb to Victoria Street
	166 Approximately

254 Approximately





	BOUNDARY ROADS – MANNINGHAM AND YARRA RANGES 


	Road
	Section
	Distance (m)

	Brushy Park Road, Wonga Park
	From Holloway Road to Homestead Road
Sealed Road
	2840




	Homestead Road, Wonga Park
	From intersection Homestead Road and Brushy Park Road
Sealed Road
	745




	Lower Homestead Road, Wonga Park
	From Reserve Road to Yarra River
Sealed Road

Unsealed Road
	585


2152 (Gravel formation)





	BOUNDARY ROADS – MAROONDAH AND YARRA RANGES 


	Road
	Section
	Distance (m)

	Liverpool Road
	Pavitt Lane to Tereddan Drive
Sealed Road

Tereddan Drive to Multi-Lanes Canterbury Road
Sealed Road
	1430


1435




	Canterbury Road
	Liverpool Road to Colchester Road
Sealed Road
	1170



	Colchester Road
	North of Canterbury Road
Sealed Road

Byron Road to Lena Grove
Sealed Road

Lena Grove to Divided Carriageway Mt. Dandenong Road
Fully Constructed Residential

Mt. Dandenong Road to Shop Car Park
Fully Constructed Residential

Shop Car Park to Byron Road
Fully Constructed Residential

	130


304


1348



42


385

	Glen Dhu Road
	Bend to Mt. Dandenong Road
Fully Constructed Residential
	420



	Ervin Road
	Marion Avenue to End
Fully Constructed Residential

South of Boundary to Boundary End
Fully Constructed Residential
	47


154



	Marion Avenue
	Hull Road to Ervin Road (Boundary Centre of Road)
Fully Constructed Residential
	495




	Hull Road
	Marion Avenue to Lincoln Road
Sealed Road
	196



	Lincoln Road
	Newman Road to Hull Road
Fully Constructed Residential
	303



	Newman Road
	Lincoln Road to Sherlock Road – Shire Boundary centre of road
Fully Constructed Residential


	674




	Maroondah Highway
	From Esther Creek to Hughes Park/Yarra Valley Golf Park

	400 Approximately




[bookmark: _Toc152584835][bookmark: _Toc204352616]4.2	Roads not listed on the Register

The following types of roads are not listed in Council’s Register of Public Roads:

· Roads which are the responsibility of the Victorian state government, statutory authority or a private owner;
· Unused roads for which Council has not accepted responsibility;
· Roads noted on a plan of subdivision, until such time as Council accepts responsibility for these roads;
· Roads which Council have not determined are reasonably required for general public use.
[bookmark: _Toc152584836]


[bookmark: _Toc204352617]Technical References

i. AS ISO 31000:2018 – Risk Management – Guidelines
ii. Integrated Asset Management Guidelines for Road Networks (AP-R202) 2002, Austroads Inc.
iii. International Infrastructure Management Manual (IIMM) 2015, IPWEA
iv. VicRoads Risk Management Guidelines
v. VicRoads Standard Specification Section 750 – Routine Maintenance
[bookmark: _Toc204352618]
Attachment 1: Road Hierarchy – Urban Roads

	Category
	Description*

	
	

	Category 1
Local Access
	These carry only local traffic. The primary function is to provide access to private properties. Key features typically include:
· Short distance travel to higher level roads
· Minimum one clear traffic lane (excluding parking)
Less than 1,000 vehicles per day


	Category 2
· Collector
	These carry significant volumes of traffic and provide access, by linking residential, commercial or industrial areas to arterial roads. They also provide links between the various collector roads. Key features typically include:
· Cater for, but may restrain, service and heavy vehicles
· Minimum two clear traffic lanes (excluding parking)


	
	



* Categories follow the Infrastructure Design Manual for residential streets


[bookmark: _Toc152584838][bookmark: _Toc204352619]Attachment 2: Road Hierarchy – Rural Roads

	Category
	Description*

	
	

	Category 1
· Local Access
	These carry only local traffic. The primary function is to provide access to private properties. Key features typically include:
· Short distance travel to higher level roads
In the case of an unsealed local access road providing access to a single property, the road will only be maintained to the closest boundary of that property. The balance will be maintained as a limited access track (see below)
· Less than 1,000 vehicles per day


	Category 2
· Collector
	These carry moderate volumes of traffic and provide access, by linking local areas to link and arterial roads. They also provide links between the various collector roads. Key features typically include:
· Cater for, but may restrain, service and heavy vehicles
· Minimum two clear traffic lanes (excluding parking)


	
	



* Categories follow the Infrastructure Design Manual for residential streets


[bookmark: _Toc204352620]Attachment 3: Pathway Hierarchy

[bookmark: _Toc167799349][bookmark: _Toc204352621]Footpaths

	Category
	Area
	Description*

	Category 1

	General-use Areas
	This category includes all other constructed Council footpaths


	Category 2

	High-use Areas
	The category of ‘highest use’ that includes all Council footpaths in shopping centres, township precincts and other pedestrian generators eg schools and railway stations.





[bookmark: _Toc167799350][bookmark: _Toc204352622]Shared & Bicycle Pathways

Shared and Bicycle pathways located in the road reserve are treated as pathways.

Shared and bicycle pathways not located in the road reserve are not subject to the Road Management Plan, refer to Council’s Paths and Trails Strategy. 


[bookmark: _Toc152584840][bookmark: _Toc204352623]Attachment 4: Inspection Requirements

	Inspection Type
	Purpose
	Inspection and Reporting Requirements

	Reactive – Request for Service (RFS)
	Reactive inspections to confirm the nature of defects/hazards reported and identify those  exceeding the intervention levels specified in Attachment 6.
	Performed by a Council/Contractor representative with knowledge of Description / Intervention Levels (Attachment 6) and road maintenance techniques. 
Higher levels of expertise may be called on if appropriate.
Reactive inspections conducted on foot, with defects measured and photographed as specified in Councils Road Asset Inspectors Manual.

The report must identify specific safety defect, time of first report, time inspected and by whom, later the subsequent action and time of completion must be added to the report.


	Proactive Inspection
	Undertaken in accord with formal programmed inspection schedule. To determine if road assets comply with the levels of service  specified.
Record of each asset is to be completed detailing:
· Name inspector
· Inspection date and
· Description of any defects that exceed intervention levels specified in Attachment 6.
In addition, details of the inspection will be electronically recorded against the particular asset inspected.

	Proactive Inspections of roads are conducted via a slow moving vehicle. Proactive Inspections of all other asset types conducted on foot, with defects measured and photographed as specified in Councils Road Asset Inspectors Manual.

[bookmark: _Hlk160717274]Performed by a dedicated Plan inspector.

	Night Inspections
	Undertaken in accord with formal programmed inspection schedule. To assess the visibility of road signage, cat’s eyes and roadside guideposts, and the visibility of line marking at night.
	Conducted via a slow moving vehicle with standard driving lights (low beam). Visibility/legibility assessed by eye from distances specified respective to each asset defect type.
Performed by a dedicated Plan inspector.




[bookmark: _Toc152584841][bookmark: _Toc204352624]Attachment 5: Inspection Frequencies

	Asset Group
	Hierarchy Category
	Reactive Inspection Timeframe
WD = Working Days
H = Hours
	Proactive Inspection Frequency
M = Months
	Night Inspections
Y = Years

	Sealed Roads
Unsealed Roads
Regulatory, Warning and Hazard Signs
	
	
	
	

	
	
	
	
	

	
	Collector 
	10 WD
	6 M
	4 Y

	
	Local 
	10 WD
	12 M
	Not carried out

	Footpaths, Kerb & Channel
	
	
	
	

	
	High Use
	5 WD
	6 M
	

	
	General
Unsealed, reactive only      
	10 WD
10 WD
	3 Y
	

	Bridges
	Level 1 Bridge Inspections
	10 WD
	12 M
	n/a

	Emergency Response – All Asset / Categories
* Reported Incidents / Hazards that present an immediate and significant risk to members of the public.
Temporary measures (e.g. installing barriers, signage, closing the road/footpath, etc.) will be implemented to reduce the risk to users of the asset until such time as appropriate repairs can be completed.
	24 H
	n/a
	n/a


* If a Proactive Inspection Frequency elapses on a Weekend or Public Holiday, the actual due date will be the next Working Day.


[bookmark: _Toc152584842][bookmark: _Toc204352625]Attachment 6: Defect Intervention Levels and Repair Timeframes

NOTES:
* If a Repair Timeframe elapses on a Weekend or Public Holiday, the compliance date will be the next Working Day.
** In cases where a defect is not due for repair within 4 weeks, temporary measures, such as installing warning signage, erecting barriers, or painting the defect with a bright contrasting colour, may be implemented at the time of identification. 

[bookmark: _Toc151559413][bookmark: _Toc152584843][bookmark: _Toc204352626]Sealed Roads
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	
	Collector
	Local

	Pothole
	Potholes in sealed pavement >70 mm in depth and >300 mm in diameter
Potholes located in dedicated/marked bicycle lanes >50 mm depth and >200 mm diameter.
	
	
	4 W
	2 M

	Edge break
	Edge breaks >300 mm laterally over a 5m or greater length from the nominal seal line or the edge line if it is line marked
	
	
	4 W
	2 M

	Edge / shoulder drop
	Edge drops onto an unsealed shoulder >100 mm in depth over a 100m or greater length
	
	
	4 W
	2 M

	Depressions / deformations
	Significant depressions or deformations in the traffic lane of a sealed pavement will be referred to Councils Capital Works Program to be prioritised in relation to available funding.
	
	
	 n/a
	 n/a

	Missing pit lids
	Missing Council drainage pit lids
	
	
	2 WD
	2 WD

	Damaged pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound)
	
	
	4 W
	2 M

	Roadside Vegetation – Overhead clearance
	· See “Vegetation Clearance Code Guidelines – Roads”
	
	
	n/a
	n/a

	
	
	
	
	 
	 

	Roadside Vegetation – Obstructing sightlines
	· See “Vegetation Clearance Code Guidelines – Roads”
	
	
	 n/a
	 n/a


[bookmark: _Toc151559414][bookmark: _Toc152584844][bookmark: _Toc204352627]Unsealed Roads
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	
	Collector
	Local

	Pothole
	Potholes in unsealed pavement >150 mm in depth and >500 mm in diameter
	
	
	1 M
	2 M

	Wheel ruts / scouring
	Wheel ruts or scouring on an unsealed road >200 mm in depth
	
	
	1 M
	2 M

	Corrugations
	Corrugations on an unsealed road will be managed in accordance with Council’s Grading Program. 
	
	
	 
	 

	Roadside Vegetation – Overhead clearance
	· See “Vegetation Clearance Code Guidelines – Roads” 
	
	
	n/a
	n/a

	
	
	
	
	 
	 

	Roadside Vegetation – Obstructing sightlines
	· See “Vegetation Clearance Code Guidelines – Roads”
	
	
	 n/a
	 n/a



1. 


[bookmark: _Toc151559415][bookmark: _Toc152584845][bookmark: _Toc204352628]Traffic Control Devices
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	
	Collector
	Local

	Missing / Damaged Signage
	Regulatory, warning and hazard signs missing, illegible or damaged making them substantially ineffective 
	
	
	2W
	2W

	Missing / Damaged Guard Rail or fencing
	Guard rail/fence damaged or missing making them substantially ineffective
	
	
	3 M
	3 M

	Missing / Damaged Pavement Markings
	Pavement markings which are missing or faded making them substantially ineffective
	
	
	15 M
	15 M



1. 

[bookmark: _Toc151559416][bookmark: _Toc152584846][bookmark: _Toc204352629]Footpaths Reactive Repairs
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	High Use
	General

	Vertical Displacement
	Vertical Displacement >30 mm in height
	 
	2 W
	2 W

	Loose segmented pavers
	Loose and unstable segmented pavers (i.e. bluestone, bricks, etc.) that move underfoot
	 
	2 W
	1 M

	Cracking
	Cracking in footpaths >40 mm wide
	 
	2 W
	1 M

	Undulations
	Undulations (depressions / bumps) >75 mm in depth/height under a 1.5m straight edge
	 
	4 W
	1 M

	Dislodged / missing pieces / potholes
	Dislodged or missing pieces or potholes >150 mm in length/width and >30 mm in depth
	 
	2 W
	1 M

	Missing pit lids
	Missing Council drainage pit lids
	 
	1 WD
	1 WD

	Damaged pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound)
	 
	2 W
	1 M

	Vegetation overhead clearance
	Vegetation intruding into the footpath envelope:
· See “Vegetation Clearance Code Guidelines – Roads” 
	 
	 n/a
	n/a

	Dislodged / missing tactile indicator
	Damaged or missing
	 
	6 W
	3 M



The times set out in the table above relate to reactive repairs.

* Pram crossings / ramps providing transition between road and footpath levels are treated as part of the footpath for the purposes of the application of description / intervention levels.




[bookmark: _Toc204352630]Footpaths Proactive Repairs
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	High Use
	General

	Vertical Displacement
	Vertical Displacement >30 mm in height
	 
	4 W
	1 M

	Loose segmented pavers
	Loose and unstable segmented pavers (i.e. bluestone, bricks, etc.) that move underfoot
	 
	4 W
	2 M

	Cracking
	Cracking in footpaths >40 mm wide
	 
	4 W
	2 M

	Undulations
	Undulations (depressions / bumps) >75 mm in depth/height under a 1.5m straight edge
	 
	6 W
	2 M

	Dislodged / missing pieces / potholes
	Dislodged or missing pieces or potholes >150 mm in length/width and >30 mm in depth
	 
	4 W
	2 M

	Missing pit lids
	Missing Council drainage pit lids
	 
	1 WD
	1 WD

	Damaged pit lids
	Damaged Council drainage pit lids (such that they are potentially structurally unsound)
	 
	4 W
	2 M

	Vegetation overhead clearance
	Vegetation intruding into the footpath envelope:
· See “Vegetation Clearance Code Guidelines – Roads” 
	
	
	

	Dislodged / missing tactile indicator
	Damaged or missing
	 
	6 W
	3 M



The times set out above relate to proactive repairs. Inspections shall be undertaken annually for each asset but divided into 4 cycles across the Council

* Pram crossings / ramps providing transition between road and footpath levels are treated as part of the footpath for the purposes of the application of description / intervention levels.

[bookmark: _Toc151559417][bookmark: _Toc152584847]

[bookmark: _Toc204352631]Kerb and Channel
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	Footpath Abutting Kerb
	
	High Use
	General

	Vertical Displacement 
	Vertical displacement – uplift where the channel meets the road pavement >50 mm
	
	
	6 M
	12 M

	Horizontal Displacement
	Horizontal displacement of the kerb from the footpath >80 mm
	
	
	6 M
	12 M






[bookmark: _Toc204352632]Bridges and Culverts
	Defect type
	Description / Intervention Level
	Repair timeframes by hierarchy
WD = Working Days
W = Weeks
M = Months

	
	
	
	
	Cat 2
	Cat 1

	Bridge & Major Culvert defects
	Visible damage likely to pose an immediate and significant risk to members of the public
	
	
	2 M
	3 M
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Figure 1. Responsibilities within the road reserve
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Figure 3. Operational Responsibility on unsealed roads





